SmartyCAM

Universal
You don’t need an AIM logger to use SmartyCAM
It can be used in all situations, with all types of vehicles.
It can source data simply from integrated GPS + three-axial
accelerometer and/or directly from a large number of ECU
via specific interfaces.
All-In-One System
The SmartyCAM captures, memorizes, compresses and reproduces your video with data overlay. Movies can easily be downloaded to your computer using a memory card, or USB cable. Watch it on your computer, or burn a DVD to watch on your TV.
Configurable Graphic Overlay
Data can be overlaid in real time to images in a virtually infinite variety of formats, with a configurable transparency level.
DVD Quality Video
SmartyCAM allows you to record digital quality movies 720x400 pixels at 30 fps with dual channel audio.
Two Audio Channel Inputs
SmartyCAM provides one internal microphone, and one input for an external microphone.
Impressive Memory Capability
On a micro-SD card, you can save hours of movies, sounds and data. The ratio is: 1 Gigabyte = 1 hour.
Compact, Handy & Easy to Install
Small (122x47, 5x46, 5mm) and lightweight (280g), SmartyCAM is very easy to install in your vehicle, using the supports included in your kit. The unit is has a waterproof rating of IP67. (see the DOWNLOADS page for Waterproof Ratings)
Image Preview
SmartyCAM allows you to view images in real time on its LCD display, allowing you to point the camera on the framing you wish—even upside down!
Rechargeable Lithium Battery
Much more convenient, cost-effective, and environmentally friendly than disposable
batteries.

Precision AutoResearch
(630) 766-4402
www.precisionautoresearch.com

Three Schematic Modes

Providing data coming from INTEGRATED GPS + THREE-AXIAL ACCELEROMETER
position
speed
acceleration
Lap time
distance
track-mapping

Providing all stand-alone data
coming from your ECU.
Supported ECU’s for use with SmartyCAM are:
AEM-EMS ver. 1.19+
Autronic SMC/SM2/SM4
BOSCH
Marelli MF4-SRA
Mercury 849849-AXX
Mitsubishi Evo X
Mustang OEM 05+
Pectal

Don’t see your ECU on the list? CONTACT US for specific instructions on how to interface SmartyCAM with your ECU.

Providing all stand-alone info + all data coming from your logger, such as:
RPM
More speeds
Lambda value (via LCU-ONE)
Engaged Gear
Temperatures
Pressures
& many more

Precision AutoResearch
(630) 766-4402
www.precisionautoresearch.com